U-Boot for Freescale i.MX27

This file contains information for the port of U-Boot to the Freescale i.MX27
SoC.

1. CONVENTIONS FOR FUSE ASSIGNMENTS
-----------------------------------

1.1 MAC Address: It is stored in the words 4 to 9 of fuse bank 0, using the
    reversed MAC byte order (i.e. LSB first).
